GEORGES  RB3    X6437                                                                                                               

EL1-1    EL NINO PERTURBATION  PROFILE          REV. 4-10-86                    

  1     6370.           EARTH RADIUS, KM (6370.)                                                                                    

  3      -1.0           TRANSMITTER HEIGHT, KM                                                                                      

  4        0.    AN KM  N. TRANSMITTER LATITUDE, KM                                                                                 

  5        0.    AN KM  E. TRANSMITTER LONGITUDE, KM                                                                                

  7      400.    FQ HZ  INITIAL FREQUENCY, HZ                                                                                       

 11       90.    AN DG  INITIAL AZIMUTH ANGLE, DEG                                                                                  

 15     -15.0    AN DG  INITIAL ELEVATION ANGLE, DEG                                                                                

 16      15.0    AN DG  FINAL   ELEVATION ANGLE, DEG                                                                                

 17       0.2    AN DG  STEP IN ELEVATION ANGLE, DEG                                                                                

 20      -1.0           RECEIVER HEIGHT, KM                                                                                         

 22       50.           MAXIMUM NUMBER OF HOPS (1.)                                                                                 

 23     1000.           MAXIMUM NUMBER OF STEPS PER HOP (1000.)                                                                     

 26        5.           MAXIMUM RAY HEIGHT, KM                                                                                      

 27       -7.           MINIMUM RAY HEIGHT, KM                                                                                      

 28      320.           MAXIMUM RANGE, KM                                                                                           

 29        0.           DO: EIGRAY/RNG-TIM/RNG-ELV/NEW-PROJ/RAYTRC/CONT/PROFL                                                       

 33   999.999           MAXIMUM ABSORPTION, DB (999.999)                                                                            

 42       1.0E-04       SINGLE-STEP INTEGRATION ERROR (1.0E-4)                                                                      

 44        .1           INITIAL INTEGRATION STEP SIZE, KM (1.0)                                                                     

 71       50.           NUMBER OF INTEGRATION STEPS PER PRINT [1.E31]                                                               

 72        1.           OUTPUT RAYSETS (1=YES; 0=NO)                                                                                

 73        0.           DIAGNOSTIC PRINTOUT (1=YES; 0=NO)                                                                           

 74        0.           PRINT RAY STEPS (0=YES; 1=N0)                                                                               

 75      .10            SMPANN LETTER HEIGHT [0.15 IN]                                                                              

 76        0.           BINARY RAY OUTPUT (1=YES; 0=NO)                                                                             

 77       57.           LINES PER PAGE IN PRINTOUT (66.)                                                                            

 81        4.           RAYPLOT PROJECTION (1=VERT, 2=HORIZ) PLANE                                                                  

 82       30.           PLOT EXPANSION FACTOR [1.]                                                                                  

 83        0.    AN KM  N. LATITUDE OF LEFT PLOT EDGE, KM                                                                           

 84        0.    AN KM  E. LONGITUDE OF LEFT PLOT EDGE, KM                                                                          

 85        0.    AN KM  N. LATITUDE OF RIGHT PLOT EDGE, KM                                                                          

 86      300.    AN KM  E. LONGITUDE OF RIGHT PLOT EDGE, KM                                                                         

 87       10.    AN KM  DISTANCE BETWEEN TIC MARKS, KM                                                                              

 88      -4.            HEIGHT ABOVE SEA LEVEL OF BOTTOM OF GRAPH, KM                                                               

 89        0.           HEIGHT ABOVE SEA LEVEL OF THE TOP OF THE GRAPH, KM                                                          

 90        1.           SOUND-SPEED PROFILE                                                                                         

 92       1.48           MINIMUM SOUND SPEED                                                                                        

 93       1.55           MAXIMUM SOUND SPEED                                                                                        

 96        1.           DISTANCE BETWEEN VERTICAL TIC MARKS, KM                                                                     

150        7.           CTANH SOUND SPEED MODEL CHECK NUMBER                                                                        

152        1.            CTANH BACKGROUND SOUND SPEED DATA SET ID                                                                   

175        3.           CBLOB3 MODEL CHECK NUMBER                                                                                   

177        1.            CBLOB3 INPUT DATA SET ID                                                                                   

178        1.            NUMBER OF BLOBS                                                                                            

179      .0149           MAX SOUND-SPEED PERTURBATION                                                                               

191      .042            VERTICAL E-FOLDING DISTANCE, KM                                                                            

275        1.           RHORIZ RECEIVER MODEL CHECK NUMBER                                                                          

300        1.           GHORIZ  TERRAIN MODEL CHECK NUMBER                                                                          

302        3.            TERRAIN DATA SET ID                                                                                        

303       -7.            HEIGHT OF TERRAIN                                                                                          

350        1.           SHORIZ MODEL CHECK NUMBER                                                                                   

352        1.            SHORIZ DATA SET ID NUMBER                                                                                  

353        0.            HEIGHT OF OCEAN SURFACE ABOVE SEA LEVEL                                                                    

 -3                     DATA SUBSET FOR BACKGROUND SOUND-SPEED MODEL                                                                

  A  EL NINO BACKGROUND SOUND-SPEED PROFILE                                                                                         

  3     999.0                                                                                                                       

   0.          1.510        0.                                                                                                      

   -.240       1.5035      -.040                                                                                                    

   -.430       1.486       -.30                                                                                                     

   -1.5        1.485       -.42                                                                                                     

   -3.0        1.508        0.                                                                                                      

   999.0                                                                                                                            

  0       RETURN TO W-ARRAY DATA SET                                                                                                

 -4                     DATA SUBSET FOR SOUND-SPEED PERTURBATION MODEL                                                              

  A  2% INCREASE IN C SQUARED AT 500 KM RANGE, 1 KM DEPTH, 150 KM WIDE                                                              

  0       RETURN TO W-ARRAY DATA SET                                                                                                

 -8                     DATA SUBSET FOR RECEIVER-SURFACE MODEL                                                                      

  A  RECEIVER SURFACE AT 1 KM BELOW SEA LEVEL                                                                                       

  0       RETURN TO W-ARRAY DATA SET                                                                                                

 -9                     DATA SUBSET FOR BACKGROUND BOTTOM MODEL                                                                     

  A  FLAT BOTTOM AT 5 KM DEPTH                                                                                                      

  0       RETURN TO W-ARRAY SUBSET                                                                                                  

179      .02             MAX SOUND-SPEED PERTURBATION                                                                               

191      .130            VERTICAL E-FOLDING DISTANCE, KM                                                                            

 -3                     DATA SUBSET FOR BACKGROUND SOUND-SPEED MODEL                                                                

  A  EL NINO BACKGROUND SOUND-SPEED PROFILE                                                                                         

  3     999.0                                                                                                                       

   0.          1.511        0.                                                                                                      

   -.240       1.5035      -.040                                                                                                    

   -.430       1.486       -.30                                                                                                     

   -1.5        1.485       -.42                                                                                                     

   -3.0        1.508        0.                                                                                                      

   999.0                                                                                                                            

  0       RETURN TO W-ARRAY DATA SET                                                                                                

 81 -4.000000    

 17  .0000000    

 29  .0000000    

 15 -13.308      1      ELEVATION ANGLE

       0

EL1-1   

 15   -.279      1      ELEVATION ANGLE

       0

EL1-1   

 15   -.190      1      ELEVATION ANGLE

       0

EL1-1   

 15 -12.498      1      ELEVATION ANGLE

       0

EL1-1   

 15  -1.044      1      ELEVATION ANGLE

       0

EL1-1   

 15   1.044      1      ELEVATION ANGLE

       0

EL1-1   

 15  12.499      1      ELEVATION ANGLE

       0

EL1-1   

 15  -8.848      1      ELEVATION ANGLE

       0

EL1-1   

 15  -2.735      1      ELEVATION ANGLE

       0

EL1-1   

 15   2.057      1      ELEVATION ANGLE

       0

EL1-1   

 15  11.415      1      ELEVATION ANGLE

       0

EL1-1   

 15  -7.567      1      ELEVATION ANGLE

       0

EL1-1   

 15  -3.962      1      ELEVATION ANGLE

       0

EL1-1   

 15   3.962      1      ELEVATION ANGLE

       0

EL1-1   

 15   7.567      1      ELEVATION ANGLE

  0

