GEORGES   RB3    X6437                                                          
N01-1     Sample Case for PC-HARPO Documentation, Rev.  6-20-90                 
  1     6370.           EARTH RADIUS TO MSL, KM (6370.)                         
  3        2.          TTRANSMITTER HEIGHT ABOVE MSL (T=ABOVE BOTTOM), KM       
  4        0.    AN KM  N. TRANSMITTER LATITUDE, KM                             
  5        0.    AN KM  E. TRANSMITTER LONGITUDE, KM                            
  7      400.    FQ HZ  INITIAL FREQUENCY, HZ                                   
 11       80.    AN DG  INITIAL AZIMUTH ANGLE, DEG                              
 15        2.    AN DG  INITIAL ELEVATION ANGLE, DEG                            
 16       16.    AN DG  FINAL   ELEVATION ANGLE, DEG                            
 17        2.    AN DG  STEP IN ELEVATION ANGLE, DEG                            
 19        0.           STOP RAYS THAT STRIKE BOTTOM (1=YES; 0=NO)              
 20       -1.           RECEIVER HEIGHT ABOVE MSL, KM                           
 22       50.           MAXIMUM NUMBER OF HOPS (1.)                             
 23     1000.           MAXIMUM NUMBER OF STEPS PER HOP (1000.)                 
 26        5.           MAXIMUM RAY HEIGHT ABOVE MSL, KM                        
 27       -5.           MINIMUM RAY HEIGHT ABOVE MSL, KM                        
 28      210.           MAXIMUM RANGE AT MSL, KM                                
 29        0.           DO: EIGRAY/RNG-TIM/RNG-ELV/NEW-PROJ/RAYTRC/CONT/PROF    
 33       20.           MAXIMUM ABSORPTION, DB (999.999)                        
 42       1.0E-06       MAXIMUM SINGLE-STEP INTEGRATION ERROR (1.0E-4)          
 44        .1           INITIAL INTEGRATION STEP SIZE, KM (1.0)                 
 57        2.           PHASE PATH  (0=NO; 1=INTEGRATE; 2=INTEGRATE/PRINT)      
 58        2.           ABSORPTION  (0=NO; 1=INTEGRATE; 2=INTEGRATE/PRINT)      
 60        2.           PATH LENGTH (0=NO; 1=INTEGRATE; 2=INTEGRATE/PRINT)      
 71       50.           NUMBER OF INTEGRATION STEPS PER PRINT [1.E9]            
 72        1.           OUTPUT RAYSETS (1=YES; 0=NO)                            
 73        0.           DIAGNOSTIC PRINTOUT (1=YES; 0=NO)                       
 74        0.           PRINT EVERY W(71) RAY STEPS (0=YES; 1=N0)               
 76        0.           BINARY RAY OUTPUT (1=YES; 0=NO)                         
 77       76.           LINES PER PAGE OF PRINTOUT = 76. FOR HPLJ (57.)         
 81        4.           RAYPLOT PROJECTION PLANE (4 = VERT. RECTANGULAR)        
 82       40.            PLOT-ORDINATE EXPANSION FACTOR [1.]                    
 83        0.    AN KM   N. LATITUDE OF LEFT PLOT EDGE, KM                      
 84        0.    AN KM   E. LONGITUDE OF LEFT PLOT EDGE, KM                     
 85      35.1    AN KM   N. LATITUDE OF RIGHT PLOT EDGE, KM                     
 86      200.    AN KM   E. LONGITUDE OF RIGHT PLOT EDGE, KM                    
 87       50.    AN KM   DISTANCE BETWEEN RANGE TICKS, KM                       
 88       -3.            HEIGHT ABOVE MSL OF BOTTOM OF GRAPH, KM                
 89        0.            HEIGHT ABOVE MSL OF TOP OF GRAPH, KM                   
 96        1.            DISTANCE BETWEEN DEPTH TICKS, KM                       
100        9.           VVORTX3 MODEL CHECK NUMBER                              
102        3.            VVORTX3 BACKGROUND CURRENT DATA SET ID                 
103      1.02    LN  M   MAXIMUM TANGENTIAL CURRENT, M/S                        
104       50.            RADIUS OF VORTEX CORE, KM                              
105        0.    AN KM   LATITUDE OF VORTEX CENTER, KM                          
106      150.    AN KM   LONGITUDE OF VORTEX CENTER, KM                         
107        1.            VERTICAL HALF-WIDTH OF VORTEX, KM                      
108       -1.            HEIGHT OF VORTEX CENTER ABOVE MSL, KM                  
125        0.           NPCURR MODEL CHECK NUMBER                               
150        7.           CTANH SOUND SPEED MODEL CHECK NUMBER                    
152        1.            CTANH BACKGROUND SOUND SPEED DATA SET ID               
175        2.           CBLOB2 SOUND SPEED PERTURBATION MODEL CHECK NUMBER      
177        7.            CBLOB2 PERTURBATION SOUND SPEED DATA SET ID            
178       .02            MAXIMUM FRACTIONAL INCREASE IN C SQUARED               
179       -1.            HEIGHT OF MAX EFFECT ABOVE MSL, KM                     
180        0.    AN KM   LATITUDE OF MAX EFFECT, KM                             
181      150.    AN KM   LONGITUDE OF MAX EFFECT, KM                            
182        1.            VERTICAL HALF-WIDTH, KM                                
183       50.    AN KM   N-S  HALF-WIDTH, KM                                    
184       50.    AN KM   E-W  HALF-WIDTH, KM                                    
275        1.           RHORIZ RECEIVER MODEL CHECK NUMBER                      
300        4.           GLORENZ BOTTOM MODEL CHECK NUMBER                       
302        3.            GLORENZ BOTTOM MODEL DATA SET ID                       
303        .5            HEIGHT OF RIDGE, KM ABOVE BASE                         
304       10.    AN KM   N. LATITUDE OF RIDGE CENTER, KM                        
305        2.    AN KM   HALF-WIDTH OF THE RIDGE, KM                            
306       -3.            HEIGHT ABOVE MSL OF BASE OF RIDGE, KM                  
325        0.           NPBOTM MODEL CHECK NUMBER                               
350        1.           SHORIZ MODEL CHECK NUMBER                               
352        1.            SHORIZ OCEAN SURFACE DATA SET ID                       
353        0.            HEIGHT OF OCEAN SURFACE ABOVE MSL, KM                  
375        0.           NPSURF MODEL CHECK NUMBER                               
500        1.           SLLOSS ABSORPTION MODEL CHECK NUMBER                    
502        1.            SLLOSS ABSORPTION DATA SET ID                          
503     0.006    AM DB   A COEFFICIENT, DB                                      
504    0.2635    AM DB   B COEFFICIENT, DB                                      
505     1000.    FQ HZ   OMEGA1, HZ                                             
506     1700.    FQ HZ   OMEGA2, HZ                                             
525        0.           NPABSRP MODEL CHECK NUMBER                              
 -1                     DATA SUBSET FOR BACKGROUND CURRENT MODEL                
  A  VORTEX AT LONGITUDE 150 KM E, UMAX= 1.02 M/S, R= 50 KM                     
  0        RETURN TO W-ARRAY DATA SET                                           
 -2                     DATA SUBSET FOR PERTURBATION CURRENT MODEL              
  A  NO CURRENT PERTURBATION                                                    
  0        RETURN TO W-ARRAY DATA SET                                           
 -3                     DATA SUBSET FOR BACKGROUND SOUND-SPEED MODEL            
  A  EL NINO BACKGROUND SOUND-SPEED PROFILE                                     
  3     999.0                                                                   
   LN  M       LN  M       LN  M                                                
   0.          1532.       0.                                                   
   -20.        1531.5      -7.                                                  
   -50.        1509.       -20.                                                 
   -250.       1503.       -40.                                                 
   -450.       1485.       -300.                                                
   -1500.      1485.       -400.                                                
   -3000.      1508.       0.                                                   
   999.0                                                                        
  0       RETURN TO W-ARRAY DATA SET                                            
 -4                     DATA SUBSET FOR SOUND-SPEED PERTURBATION MODEL          
  A  2% INCREASE IN C-SQUARED AT 150 KM LON., 1 KM DEPTH, 50 KM WIDE            
  0       RETURN TO W-ARRAY DATA SET                                            
 -8                     DATA SUBSET FOR RECEIVER-SURFACE MODEL                  
  A  RECEIVER SURFACE = SPHERE 1 KM BELOW MSL                                   
  0       RETURN TO W-ARRAY DATA SET                                            
 -9                     DATA SUBSET FOR BACKGROUND BOTTOM MODEL                 
  A  RIDGE .5 KM HIGH, 2 KM WIDE AT 10 KM N LATITUDE; BASE= -3 KM               
  0       RETURN TO W-ARRAY DATA SET                                            
-10                     DATA SUBSET FOR BOTTOM PERTURBATION MODEL               
  A  NO BOTTOM PERTURBATION                                                     
  0       RETURN TO W-ARRAY DATA SET                                            
-11                     DATA SUBSET FOR OCEAN SURFACE MODEL                     
  A  OCEAN SURFACE = SPHERE AT MSL                                              
  0       RETURN TO W-ARRAY DATA SET                                            
-12                     DATA SUBSET FOR OCEAN SURFACE PERTURBATION MODEL        
  A  NO OCEAN SURFACE PERTURBATION                                              
  0       RETURN TO W-ARRAY DATA SET                                            
-17                     DATA SUBSET FOR OCEAN ABSORPTION MODEL                  
  A  SKRETTING-LEROY ABSORPTION FORMULA                                         
  0       RETURN TO W-ARRAY DATA SET                                            
-18                     DATA SUBSET FOR PERTURBATION ABSORPTION MODEL           
  A  NO ABSORPTION PERTURBATION                                                 
  0       RETURN TO W-ARRAY DATA SET                                            
  0                     **********  END OF RUN SET NUMBER 1  *********          
N01-2     Sample Case for PC-HARPO Documentation, Rev.  6-20-90                 
 71        0.           NUMBER OF INTEGRATION STEPS PER PRINT [1.E9]            
 72        0.           OUTPUT RAYSETS (1=YES; 0=NO)                            
 73        1.           DIAGNOSTIC PRINTOUT (1=YES; 0=NO)                       
 81        2.           RAYPLOT PROJECTION PLANE (2 = HORIZONTAL)               
 88       -1.           HEIGHT OF HORIZONTAL PLOT SECTION ABOVE MSL, KM         
  0                     **********  END OF RUN SET NUMBER 2  *********          
****SOFT EOF***+++++
N01-1     Sample Case for PC-HARPO Documentation, Rev.  6-20-90                  7/ 1/1990     0h 4m  
VVORTX3     3.0 NPCURR       .0   CTANH       1.0 CBLOB2      7.0
GLORENZ     3.0 NPBOTM       .0   SLLOSS      1.0 NPABSR       .0
RHORIZ       .0 SHORIZ      1.0   NPSURF       .0
  VORTEX AT LONGITUDE 150 KM E, UMAX= 1.02 M/S, R= 50 KM                        
  NO CURRENT PERTURBATION                                                       
  EL NINO BACKGROUND SOUND-SPEED PROFILE                                        
  2% INCREASE IN C-SQUARED AT 150 KM LON., 1 KM DEPTH, 50 KM WIDE               
  RIDGE .5 KM HIGH, 2 KM WIDE AT 10 KM N LATITUDE; BASE= -3 KM                  
N013    -9808     0     0   -10000 25132741   8000000    200000        0   0 50T
   -10000   194734   -18   -20 -2022   1311291   1311291   288     0   0   0  1R
   -10000   520417   -16   -27  2010   3504472   3504471   769     0   0   0  2R
   -10000   723109   -15   -42 -1990   4868914   4868914  1069     0   0   0  3R
   -10000  1127595     6  -147  1418   7586966   7586966  1667     0   0   0  4R
   -10000  1406506    51  -324 -1281   9454219   9454219  2079     0   0   0  5R
   -10000  1941240   197  -503  3128  13036463  13036463  2870     0   0   0  6R
    -8511  2101960   240  -509 -2971  14116463  14116463  3108     0   0   0  7F
N013    -9808     0     0   -10000 25132741   8000000    400000        0   0 50T
   -10000   165446   -17   -19 -4012   1114351   1114351   245     0   0   0  1R
   -10000   468372   -15   -22  4001   3154502   3154502   693     0   0   0  2R
   -10000   637278   -14   -31 -3985   4291986   4291986   943     0   0   0  3R
   -10000   963209    -6   -74  3618   6484653   6484653  1425     0   0   0  4R
   -10000  1149018     7  -148 -3476   7731899   7731898  1700     0   0   0  5R
   -10000  1652653    91  -346  2658  11104455  11104455  2446     0   0   0  6R
   -10000  1864722   142  -439 -2819  12525535  12525535  2759     0   0   0  7R
   -15734  2105919   200  -455  1823  14145535  14145535  3116     0   0   0  8F
N013    -9808     0     0   -10000 25132741   8000000    600000        0   0 50T
   -10000   145209   -16   -17 -6008    978585    978585   215     0   0   0  1R
   -10000   458199   -12   -18  5996   3086200   3086200   679     0   0   0  2R
   -10000   605599   -13   -25 -5983   4079462   4079462   898     0   0   0  3R
   -10000   934379    -6   -55  5593   6291447   6291447  1385     0   0   0  4R
   -10000  1090494     1  -108 -5472   7340500   7340500  1616     0   0   0  5R
   -10000  1530604    52  -242  4301  10289292  10289292  2268     0   0   0  6R
   -10000  1709365    87  -352 -4402  11486110  11486110  2533     0   0   0  7R
   -10000  2087795   168  -388  5537  14026691  14026691  3093     0   0   0  8R
    -8578  2102600   171  -389  5404  14126691  14126691  3115     0   0   0  9F
N013    -9808     0     0   -10000 25132741   8000000    800000        0   0 50T
   -10000   134059   -15   -16 -8006    904047    904047   199     0   0   0  1R
   -10000   482230    -9   -14  7989   3246733   3246733   716     0   0   0  2R
   -10000   617971   -10   -22 -7975   4162042   4162042   918     0   0   0  3R
   -10000   980715    -4   -48  7435   6600587   6600587  1456     0   0   0  4R
   -10000  1123615     2  -102 -7311   7561098   7561098  1669     0   0   0  5R
   -10000  1557112    45  -192  6434  10465570  10465570  2312     0   0   0  6R
   -10000  1710190    69  -283 -6530  11491347  11491347  2539     0   0   0  7R
   -10281  2100554   134  -300  7721  14111347  14111347  3118     0   0   0  8F
N013    -9808     0     0   -10000 25132741   8000000   1000000        0   0 50T
   -10000   193456   -12   -14-10005   1298480   1298480   288     0   0   0  1R
   -28979   348791    -9   232  3400   2345757   2345757   519     0   0   0  2G
   -10000   493788   -80   159 10224   3324473   3324474   735     0   0   0  2R
   -10000   670788  -126   105-10188   4513905   4513905   999     0   0   0  3R
   -28954   811497  -145  -210  3021   5464007   5464008  1209     0   0   0  4G
   -10000   964893  -113  -197  9505   6497632   6497633  1437     0   0   0  4R
   -10000  1176220   -76  -234 -9212   7911470   7911470  1751     0   0   0  5R
   -29882  1322094   -48  -265  4554   8894430   8894430  1969     0   0   0  6G
   -10000  1471174   -19  -295  8695   9897927   9897927  2191     0   0   0  6R
   -10000  1700700    31  -383 -8865  11429294  11429295  2532     0   0   0  7R
   -29961  1861151    68  -394  3353  12508746  12508747  2771     0   0   0  8G
   -10000  2017061   100  -384  9692  13559231  13559232  3004     0   0   0  8R
    -1257  2100424   117  -384  1425  14119231  14119232  3128     0   0   0  9F
N013    -9808     0     0   -10000 25132741   8000000   1200000        0   0 50T
   -10000   116447   -13   -14-12004    788973    788973   175     0   0   0  1R
   -29508   227433   -10   193  7184   1543215   1543216   341     0   0   0  2G
   -10000   335994   -75   127 12169   2281500   2281500   504     0   0   0  2R
   -10000   450772  -111    88-12165   3059732   3059733   676     0   0   0  3R
   -25790   532686  -127  3158 11314   3619144   3619144   800     0   0   0  4G
   -10000   600692  -486  2797 14060   4087894   4087895   903     0   0   0  4R
   -10000   699780  -885  2392-14041   4763564   4763565  1053     0   0   0  5R
   -27472   776090 -1122  -362  8925   5288367   5288368  1169     0   0   0  6G
   -10000   864716 -1086  -335 12427   5893266   5893268  1302     0   0   0  6R
   -10000   974114 -1050  -323-12356   6635033   6635035  1467     0   0   0  7R
   -29598  1074338 -1020  -497  8489   7317761   7317763  1617     0   0   0  8G
   -10000  1177288  -977  -482 11826   8017840   8017842  1772     0   0   0  8R
   -10000  1290483  -934  -502-11733   8782483   8782485  1942     0   0   0  9R
   -29865  1392201  -896  -541  9044   9474203   9474204  2095     0   0   0 10G
   -10000  1494738  -858  -546 11543  10171061  10171063  2250     0   0   0 10R
   -10000  1609212  -816  -582-11578  10943305  10943306  2422     0   0   0 11R
   -29935  1713287  -778  -596  8749  11650537  11650538  2578     0   0   0 12G
   -10000  1816361  -743  -591 11929  12351703  12351704  2733     0   0   0 12R
   -10000  1928983  -706  -597-12030  13113644  13113645  2902     0   0   0 13R
   -29962  2035948  -673  -588  7919  13840989  13840989  3063     0   0   0 14G
   -18778  2100987  -655  -572 11474  14280989  14280989  3161     0   0   0 14F
N013    -9808     0     0   -10000 25132741   8000000   1400000        0   0 50T
   -10000    96474   -13   -14-14003    657818    657818   146     0   0   0  1R
   -29600   185493   -10   206 10186   1267978   1267978   280     0   0   0  2G
   -10000   273220   -79   137 14155   1869704   1869704   413     0   0   0  2R
   -10000   374756  -120    94-14153   2560890   2560890   567     0   0   0  3R
   -27790   452665  -138  2653 12635   3096309   3096309   685     0   0   0  4G
   -10000   521548  -491  2300 15588   3573382   3573382   790     0   0   0  4R
        0   562926  -661  2128 -6517   3858025   3858026   853     0   0   0  5A
   -10000   604317  -808  1979-15580   4142711   4142711   916     0   0   0  5R
   -25168   661771  -981  -413 11913   4541478   4541479  1004     0   0   0  6G
   -10000   725091  -947  -383 14335   4978134   4978134  1100     0   0   0  6R
        0   773854  -924  -365 -2616   5310488   5310489  1174     0   0   0  7A
   -10000   822672  -904  -351-14302   5643124   5643125  1248     0   0   0  7R
   -29130   905056  -872 -1030 10348   6209075   6209075  1373     0   0   0  8G
   -10000   991598  -784  -956 13622   6801934   6801935  1504     0   0   0  8R
   -10000  1091722  -697  -904-13547   7482368   7482369  1655     0   0   0  9R
   -29775  1180022  -629  -958 10589   8087007   8087008  1788     0   0   0 10G
   -10000  1269610  -561  -922 13183   8699639   8699640  1924     0   0   0 10R
   -10000  1373491  -490  -917-13126   9402993   9402995  2081     0   0   0 11R
   -29904  1462585  -433  -926 10886  10012246  10012248  2216     0   0   0 12G
   -10000  1551897  -379  -910 13086  10622890  10622893  2351     0   0   0 12R
   -10000  1655342  -319  -919-13134  11323316  11323318  2507     0   0   0 13R
   -29948  1745912  -269  -914 10549  11942496  11942499  2644     0   0   0 14G
   -10000  1835857  -224  -893 13413  12558001  12558004  2780     0   0   0 14R
   -10000  1935470  -175  -882-13489  13234962  13234965  2930     0   0   0 15R
   -29968  2027494  -134  -862  9968  13864530  13864534  3069     0   0   0 16G
   -14448  2100720  -104  -837 13577  14364530  14364534  3180     0   0   0 16F
N013    -9808     0     0   -10000 25132741   8000000   1600000        0   0 50T
        0    39152   -13   -14 -7420    269703    269703    60     0   0   0  1A
   -10000    78975   -13   -14-16003    544103    544103   120     0   0   0  1R
   -29653   153961   -10   213 12811   1063042   1063042   235     0   0   0  2G
   -10000   228151   -83   140 16139   1576821   1576820   348     0   0   0  2R
        0   267475  -105   117 -7714   1847998   1847998   408     0   0   0  3A
   -10000   306799  -122    99-16138   2119176   2119176   468     0   0   0  3R
   -28791   377222  -143  1485 13972   2607306   2607306   576     0   0   0  4G
   -10000   443760  -367  1260 16889   3070471   3070471   678     0   0   0  4R
        0   480587  -465  1161 -9230   3325562   3325562   735     0   0   0  5A
   -10000   517418  -549  1075-16886   3580665   3580664   791     0   0   0  5R
   -25573   571345  -652  5462 16468   3957184   3957184   874     0   0   0  6G
   -10000   619964 -1083  5030 18383   4300867   4300866   950     0   0   0  6R
        0   652683 -1337  4774-11851   4530267   4530267  1001     0   0   0  7A
   -10000   685421 -1566  4543-18376   4759688   4759688  1052     0   0   0  7R
   -25168   732669 -1861  1370 15683   5093370   5093369  1125     0   0   0  8G
   -10000   782658 -1950  1277 17518   5443729   5443728  1202     0   0   0  8R
        0   817521 -2005  1217-10579   5685999   5685998  1256     0   0   0  9A
   -10000   852403 -2056  1161-17499   5928338   5928337  1310     0   0   0  9R
   -28039   912552 -2133 -1725 13679   6348794   6348792  1403     0   0   0 10G
   -10000   978766 -2017 -1620 16051   6808190   6808188  1504     0   0   0 10R
        0  1017652 -1956 -1571 -8326   7076045   7076043  1563     0   0   0 11A
   -10000  1056589 -1899 -1527-16008   7344119   7344117  1623     0   0   0 11R
   -29512  1128133 -1803 -1841 13397   7839875   7839872  1733     0   0   0 12G
   -10000  1201295 -1691 -1752 15561   8345838   8345835  1844     0   0   0 12R
        0  1241192 -1635 -1718 -8086   8619674   8619671  1905     0   0   0 13A
   -10000  1281144 -1581 -1688-15517   8893751   8893748  1966     0   0   0 13R
   -29809  1354746 -1489 -1724 13598   9402668   9402664  2079     0   0   0 14G
   -10000  1428894 -1399 -1666 15337   9914954   9914949  2192     0   0   0 14R
        0  1469161 -1353 -1648 -8082  10190808  10190803  2254     0   0   0 15A
   -10000  1509431 -1309 -1632-15335  10466671  10466666  2315     0   0   0 15R
   -29902  1583933 -1231 -1623 13562  10981354  10981349  2429     0   0   0 16G
   -10000  1658384 -1157 -1578 15416  11495851  11495845  2543     0   0   0 16R
        0  1698664 -1119 -1565 -7923  11772004  11771998  2605     0   0   0 17A
   -10000  1738890 -1082 -1551-15459  12047914  12047908  2666     0   0   0 17R
   -29941  1814326 -1016 -1525 13200  12569117  12569111  2781     0   0   0 18G
   -10000  1889434  -955 -1482 15669  13088524  13088517  2896     0   0   0 18R
        0  1929544  -923 -1464 -7663  13364155  13364148  2957     0   0   0 19A
   -10000  1969598  -893 -1446-15715  13639529  13639522  3018     0   0   0 19R
   -29961  2045749  -838 -1412 12804  14166026  14166018  3135     0   0   0 20G
   -15880  2100885  -801 -1378 15626  14546026  14546017  3219     0   0   0 20F
                                                                              -
N01-2     Sample Case for PC-HARPO Documentation, Rev.  6-20-90                  7/ 1/1990     0h 4m  
VVORTX3     3.0 NPCURR       .0   CTANH       1.0 CBLOB2      7.0
GLORENZ     3.0 NPBOTM       .0   SLLOSS      1.0 NPABSR       .0
RHORIZ       .0 SHORIZ      1.0   NPSURF       .0
  VORTEX AT LONGITUDE 150 KM E, UMAX= 1.02 M/S, R= 50 KM                        
  NO CURRENT PERTURBATION                                                       
  EL NINO BACKGROUND SOUND-SPEED PROFILE                                        
  2% INCREASE IN C-SQUARED AT 150 KM LON., 1 KM DEPTH, 50 KM WIDE               
  RIDGE .5 KM HIGH, 2 KM WIDE AT 10 KM N LATITUDE; BASE= -3 KM                  
