MIKE=JONES=RL3=X6464

0T6  MUNK'S 1974 UNIFORM SOUND CHANNEL WITH VVORTEX CURRENT MODEL 3

 29 1.                  1=PROCESS PROFILE RUNSET, 0=SKIP RUNSET

 83 0.           AN KM  LEFT LATITUDE OF PLOT, KM

 84 0.           AN KM  LEFT LONGITUDE OF PLOT, KM

 88-5.00000000000       HEIGHT ABOVE SEA LEVEL OF BOTTOM OF GRAPH, KM

 89 0.                  HEIGHT ABOVE SEA LEVEL OF THE TOP OF THE GRAPH

 90 1.00000000000       SELECT SOUND SPEED

 92 1.49000000000       HORIZONTAL AXIS MINIMUM

 93 1.54000000000       HORIZONTAL AXIS MAXIMUM

 94 .010000000000LN KM  HORIZONTAL AXIS TICK MARK INTERVAL

 96 1.00000000000       DISTANCE BETWEEN VERTICAL TICK MARKS, KM

100        9.           VVORTX3 MODEL CHECK NUMBER

 -1                     DATA SUBSET FOR BACKGROUND CURRENT MODEL

  A  VORTEX AT LONGITUDE 150 KM E, UMAX= 1.02 M/S, R= 50 KM

  0        RETURN TO W-ARRAY DATA SET

102        3.            VVORTX3 BACKGROUND CURRENT DATA SET ID

103      1.02    LN  M   MAXIMUM TANGENTIAL CURRENT, M/S

104       50.            RADIUS OF VORTEX CORE, KM

105        0.    AN KM   LATITUDE OF VORTEX CENTER, KM

106      150.    AN KM   LONGITUDE OF VORTEX CENTER, KM

107        1.            VERTICAL HALF-WIDTH OF VORTEX, KM

108       -1.            HEIGHT OF VORTEX CENTER ABOVE MSL, KM

125        0.           NPCURR MODEL CHECK NUMBER

 -2                     DATA SUBSET FOR PERTURBATION CURRENT MODEL

  A  NO CURRENT PERTURBATION

  0        RETURN TO W-ARRAY DATA SET

150 5.00000000000       CSMUNK1 SOUND SPEED MODEL 

152 2.00000000000       INPUT DATA SET ID NUMBER

153 1.00000000000       REFERENCE SOUND SPEED

154 0.           AN KM  PH1 LONGITUDE 1 

155 1.49200000000       CA1 SOUND SPEED ON AXIS

156-1.30000000000       ZA1 DEPTH OF AXIS

157 1.30000000000       H1 SCALE DEPTH

158 .007400000000       EP1 FRACTIONAL INCREASE OF C WITH DEPTH

159 1000.00000000AN KM  PH2 LONGITUDE 2 

160 1.49200000000       CA2 SOUND SPEED ON AXIS

161-1.30000000000       ZA2 DEPTH OF AXIS

162 1.30000000000       H2 SCALE DEPTH

163 .007400000000       EP2 FRACTIONAL INCREASEE OF C WITH DEPTH

175 0.0                 NPSPEED - DO NOTHING SPEED PERTURBATION MODEL

200 1.0                 TLINEAR MODEL CHECK NUMBER

201 1.                  DATA FORMAT CODE

202 1.                  DATA SET ID NUMBER

203 293.                BOTTOM TEMPERATURE, DEGREES KELVIN

204 2.3                 TEMPERATURE GRADIENT, DEGREES KELVIN/KM

225 0.                  NPTEMP, DO-NOTHING TEMPERATURE PERTURBATION

275 1.00000000000       RHORIZ RECEIVER MODEL CHECK NUMBER

300        4.           GLORENZ BOTTOM MODEL CHECK NUMBER

302        3.            GLORENZ BOTTOM MODEL DATA SET ID

303        .5            HEIGHT OF RIDGE, KM ABOVE BASE

304       10.    AN KM   N. LATITUDE OF RIDGE CENTER, KM

305        2.    AN KM   HALF-WIDTH OF THE RIDGE, KM

306       -3.            HEIGHT ABOVE MSL OF BASE OF RIDGE, KM

325        0.            DO-NOTHING BOTTOM PERTURBATION

  0

0T6    SAMPLE SOUND SPEED DATA POINTS

 90-42.0000000000       NEGATIVE VALUE INDICATES SUPERIMPOSE DATA POINTS

-42                     ENTERING DATA SUBSET

  2      999.0

   LN KM        LN KM

 -.568240E-01  1.53400

 -.710503E-01  1.53282

 -.853171E-01  1.53165

 -.995969E-01  1.53048

 -.113850      1.52931

 -.128006      1.52814

 -.141939      1.52697

 -.155372      1.52581

 -.167350      1.52464

 -.177608      1.52348

 -.195094      1.52232

 -.212698      1.52117

 -.230376      1.52001

 -.248050      1.51886

 -.265561      1.51770

 -.282521      1.51655

 -.297255      1.51540

 -.313064      1.51426

 -.335598      1.51311

 -.358481      1.51197

 -.381655      1.51082

 -.404971      1.50968

 -.428009      1.50854

 -.448662      1.50741

 -.471800      1.50627

 -.503609      1.50514

 -.536853      1.50401

 -.571848      1.50288

 -.609165      1.50175

 -.650365      1.50062

 -.698865      1.49950

 -.733760      1.49837

 -.770014      1.49725

 -.806911      1.49613

 -.841016      1.49501

 -.843638      1.49390

 -.941190      1.49278

 -4.32248      1.53400

 -4.26850      1.53282

 -4.21328      1.53165

 -4.15665      1.53048

 -4.09840      1.52931

 -4.03821      1.52814

 -3.97557      1.52697

 -3.90943      1.52581

 -3.83637      1.52464

 -3.75539      1.52348

 -3.69719      1.52232

 -3.63710      1.52117

 -3.57480      1.52001

 -3.50979      1.51886

 -3.44119      1.51770

 -3.36717      1.51655

 -3.28030      1.51540

 -3.19451      1.51426

 -3.13375      1.51311

 -3.07037      1.51197

 -3.00377      1.51082

 -2.93298      1.50968

 -2.85600      1.50854

 -2.76490      1.50742

 -2.67538      1.50627

 -2.45335      1.50288

 -2.36103      1.50175

 -2.24327      1.50062

 -2.06858      1.49950

 -2.03932      1.49837

 -2.01206      1.49725

 -1.99054      1.49613

 -1.98684      1.49501

 -2.08138      1.49390

 -1.97047      1.49278

  999.000

  0                     RETURNING TO W ARRAY DATA SET

  0

0T6    SAMPLE SOUND SPEED DATA POINTS

 90-41.0000000000       NEGATIVE VALUE = SUPERIMPOSE ON PREVIOUS PLOT

-41                     NEGATIVE VALUE = TABULAR DATA SET FOLLOWS

  2      999.0

   LN KM        LN KM

 -2.66103      1.51175

 -2.54327      1.51062

 -2.40858      1.50950

 -2.40932      1.50837

 -2.40206      1.50725

 -2.38054      1.50613

 -2.28684      1.50501

 -2.30138      1.50390

 -2.27047      1.50278

  999.000

  0                     RETURNING TO W ARRAY DATA SET

  0

0T6  MUNK'S 1974 UNIFORM SOUND CHANNEL WITH VVORTEX CURRENT MODEL 3

 29 1.0000              1 = PROFILE, 0 = SKIP THIS RUNSET

 83 5.           AN KM  Latitude of the profile   (rad, deg, km) north (W83)

 84 145.         AN KM  Longitude of the profile   (rad, deg, km) east (W84)

 88-5.00000000000       Height above sea level of bottom of graph   km (W88)

 89 0.                  HEIGHT ABOVE SEA LEVEL OF TOP OF GRAPH

 90 2.00000000000       CURRENT SPEED

 92 0.00000000000       Minimum speed km/s, m/s (auto-scaling if zero)

 93 0.00000000000       Maximum speed km/s, m/s (auto-scaling if zero)

 94 0.00000000000       Horizontal tick mark interval km/s, m/s (auto-scaling if zero)

 96 1.00000000000       Vertical tick mark interval km (auto-scaling if zero)

  0

0T6  MUNK'S 1974 UNIFORM SOUND CHANNEL WITH VVORTEX CURRENT MODEL 3

 29 1.0000              1 = PROFILE, 0 = SKIP THIS RUNSET

 83 5.           AN KM  Latitude of the profile   (rad, deg, km) north

 84 145.         AN KM  Longitude of the profile   (rad, deg, km) east

 88-5.00000000000       Height above sea level of bottom of graph   km

 89    0.               Height above sea level of top of graph  km

 90 4.00000000000       SOUTHWARD component of current velocity

 92 0.00000000000       Minimum speed km/s, m/s (auto-scaling if zero)

 93 0.00000000000       Maximum speed km/s, m/s (auto-scaling if zero)

 94 0.00000000000       Horizontal tick mark interval km/s, m/s (auto-scaling if zero)

 96 0.00000000000       Vertical tick mark interval km (auto-scaling if zero)

  0

0T6  MUNK'S 1974 UNIFORM SOUND CHANNEL WITH VVORTEX CURRENT MODEL 3

 29 1.0000              1 = PROFILE, 0 = SKIP THIS RUNSET

 83 5.           AN KM  Latitude of the profile  (rad, deg, km) north

 84 145.         AN KM  Longitude of the profile  (rad, deg, km) east

 88-5.00000000000       Height above sea level of bottom of graph  km

 89 0.                  Height above sea level of top of graph  km

 90 5.00000000000	EASTWARD component of current velocity

 92 0.00000000000       Minimum speed  km/s, m/s (auto-scaling if zero)

 93 0.00000000000       Maximum speed  km/s, m/s (auto-scaling if zero)

 94 0.00000000000       Horizontal tick mark interval km/s, m/s (auto-scaling if zero)

 96 1.00000000000	Vertical tick mark interval km (auto-scaling if zero)

 0

0T6    TLINEAR TEMPERATURE PROFILE

 29 1.0000              1 = PROFILE, 0 = SKIP THIS RUNSET

 83 5.           AN KM  Latitude of the profile   (rad, deg, km) north

 84 145.         AN KM  Longitude of the profile   (rad, deg, km) east

 88 0.00000000000       Height above sea level of bottom of graph   km

 89    3.               Height above sea level of top of graph  km

 90 7.00000000000       TEMPERATURE PROFILE

 92 290.000000000       Minimum temperature deg K (auto-scaling if zero)

 93 300.000000000       Maximum temperature deg K (auto-scaling if zero)

 94 0.00000000000       Horizontal tick mark interval deg K (auto-scaling if zero)

 96 0.00000000000	Vertical tick mark interval km (auto-scaling if zero)

   0

0T6    SAMPLE TEMPERATURE DATA POINTS

 90-45.0000000000       NEGATIVE VALUE = SUPERIMPOSE ON PREVIOUS PLOT

-45                     NEGATIVE VALUE = TABULAR DATA SET FOLLOWS

  2      999.0

 1.06103      295.1175

 1.04327      295.1062

 1.00858      295.0950

 1.10932      295.0837

 1.20206      295.0725

 1.38054      296.0613

 1.28684      296.0501

 1.40138      296.0390

 1.47047      296.0278

  999.000

  0                     RETURNING TO W ARRAY DATA SET

  0

0T6    GLORENZ TOPOGRAPHY PROFILE

 29 1.0000              1 = PROFILE, 0 = SKIP THIS RUNSET

 83 0.           AN KM  Left Latitude of plot   (rad, deg, km) north

 84 0.           AN KM  Longitude of plot  (rad, deg, km) east

 85 20.          AN KM  Right Latitude of plot  (rad, deg, km) north

 90 6.00000000000       TOPOGRAPHY PROFILE

  0

